**BOAT SPECIFICATION**

|  |  |  |  |
| --- | --- | --- | --- |
| **Number** | **Description of requirement** | **Unit** | **Qty** |
| 1 | **Boat W23S body made of fibre glass and Aluminium, with Sunshades framing with plastic canopy covering, 4 benches,  Loading capacity 1000Kgs , 12 pax max,+ Driver** | pc | 1 |
| 2 | **2-Stroke Outboard Engine 75HP**  (With 3-cylinder engine type,3-carburator fuel induction system, tiller handle steering, pre-mixing lubrication, manual starter system, CDI ignition system, Fuel tanker minimum 25litr siz , fuel line, manual, engine hour-meter PET-3200R ). | pc | 1 |
| 3 | Anchor Complete 8kgs | pc | 2 |
| 4 | Vest - buoyancy aid (Life Jacket) Green colousr | pc | 20 |
| 5 | Life Rings 30" x 2.5kg | pc | 2 |
| 6 | Fire Extinguisher 1kg Dry Powder | pc | 2 |
| 7 | First Aid Kit Medium | pc | 2 |
| 8 | Fire Blanket 4'X4' | pc | 2 |
| 9 | Paddle aluminium handle, blade & cap | pc | 4 |
| 10 | Spare part for one-year standard operations: 4 No. fuel filter Assy, 3 No. water separator, 200 litres of Outboard 2 stroke motor oil, 15 litres of Motor Gear Oil API-4SAE90, 3 No. Spark Plug B8HS-10, 2 No. Gasket washer, 2 No. whistles and 2 No. propellers. | Lump Sum | 1 |

****